FIRE ALARM SYSTEM MONTHLY TEST RECORD

Every month the following tests shall be conducted and if a fault is established appropriate corrective action shall be taken. (Initial each area.)

Month	(A)

Manual Pull Stations	(B)

Bells	(C) Annunciator	(D)

Trouble Signal	(E)

Battery Condition	Date

(mm/dd/yy)	Signature
January

February

March

April

May

June

July

August

September

October

November

December

(A)	One (1) alarm initiating pull station device shall be operated on a rotational basis and shall initiate an alarm condition.

(B)	Intended function of all alarm audible signal appliances (bells) shall be ensured.

(C)	The annunciator panel shall be checked to ensure that the tested devices annunciate correctly.

(D)	Intended function of audible and visual trouble signals shall be ensured.

(E)	Fire alarm batteries shall be visually inspected.

Anubis

s y s t e m s t e c h n o l o g i e s